Overview | Package | Class | Use | Tree | Deprecated | Index | Help
| " 2013 FRC Java API "
PREV CLASS NEXT CLASS | FRAMES NO FRAMES
SUMMARY: NESTED | FIELD | CONSTR | METHOD | DETAIL: FIELD | CONSTR | METHOD

## edu.wpi.first.wpilibj
Interface Sendable

All Known Subinterfaces:
  LiveWindowSendable, NamedSendable

All Known Implementing Classes:
  Accelerometer, AnalogChannel, AnalogIOButton, AnalogPotentiometer, Button, CANJaguar, Command, CommandGroup, Compressor, Counter, DigitalInput, DigitalIOButton, DigitalOutput, DoubleSolenoid, Encoder, GearTooth, Gyro, HiTechnicColorSensor, HiTechnicCompass, InternalButton, Jaguar, JoystickButton, NetworkButton, PIDCommand, PIDController, PIDSubsystem, PrintCommand, PWM, Relay, SafePWM, Scheduler, SendableChooser, Servo, Solenoid, StartCommand, Subsystem, Talon, Trigger, Ultrasonic, Victor, WaitCommand, WaitForChildren, WaitUntilCommand

    public interface Sendable

The base interface for objects that can be sent over the network through network tables.

Method Summary
`String` | `getSmartDashboardType()`
`ITable` | `getTable()`
`void` | `initTable(ITable subtable)` Initializes a table for this sendable object.

Method Detail

### initTable

    void initTable(ITable subtable)

  Initializes a table for this sendable object.

  Parameters:
    `subtable` - The table to put the values in.

### getTable

    ITable getTable()

  Returns:
    the table that is currently associated with the sendable

### getSmartDashboardType

    String getSmartDashboardType()

  Returns:
    the string representation of the named data type that will be used by the smart dashboard for this sendable

Overview | Package | Class | Use | Tree | Deprecated | Index | Help
| " 2013 FRC Java API "
PREV CLASS NEXT CLASS | FRAMES NO FRAMES
SUMMARY: NESTED | FIELD | CONSTR | METHOD | DETAIL: FIELD | CONSTR | METHOD

"
For updated information see the Java FRC site
"