Overview | Package | Class | Use | Tree | Deprecated | Index | Help
| " 2013 FRC Java API "
PREV NEXT | FRAMES NO FRAMES

## Uses of Class
edu.wpi.first.wpilibj.Relay.Direction

Packages that use Relay.Direction
edu.wpi.first.wpilibj | The WPI Robotics library (WPILibJ) is a set of Java classes that interfaces to the hardware in the FRC control system and your robot.

Uses of Relay.Direction in edu.wpi.first.wpilibj

Fields in edu.wpi.first.wpilibj declared as Relay.Direction
`static Relay.Direction` | `Relay.Direction.kBoth` direction: both directions are valid
`static Relay.Direction` | `Relay.Direction.kForward` direction: Only forward is valid
`static Relay.Direction` | `Relay.Direction.kReverse` direction: only reverse is valid

Methods in edu.wpi.first.wpilibj with parameters of type Relay.Direction
`void` | `Relay.setDirection(Relay.Direction direction)` Set the Relay Direction Changes which values the relay can be set to depending on which direction is used Valid inputs are kBothDirections, kForwardOnly, and kReverseOnly

Constructors in edu.wpi.first.wpilibj with parameters of type Relay.Direction
`Relay(int moduleNumber, int channel, Relay.Direction direction)` Relay constructor given the module and the channel.
`Relay(int channel, Relay.Direction direction)` Relay constructor given a channel only where the default digital module is used.

Overview | Package | Class | Use | Tree | Deprecated | Index | Help
| " 2013 FRC Java API "
PREV NEXT | FRAMES NO FRAMES

"
For updated information see the Java FRC site
"