Overview | Package | Class | Use | Tree | Deprecated | Index | Help
| " 2013 FRC Java API "
PREV NEXT | FRAMES NO FRAMES

## Uses of Class
edu.wpi.first.wpilibj.Relay.Value

Packages that use Relay.Value
edu.wpi.first.wpilibj | The WPI Robotics library (WPILibJ) is a set of Java classes that interfaces to the hardware in the FRC control system and your robot.

Uses of Relay.Value in edu.wpi.first.wpilibj

Fields in edu.wpi.first.wpilibj declared as Relay.Value
`static Relay.Value` | `Relay.Value.kForward` value: forward
`static Relay.Value` | `Relay.Value.kOff` value: off
`static Relay.Value` | `Relay.Value.kOn` value: on for relays with defined direction
`static Relay.Value` | `Relay.Value.kReverse` value: reverse

Methods in edu.wpi.first.wpilibj that return Relay.Value
`Relay.Value` | `Relay.get()` Get the Relay State Gets the current state of the relay.

Methods in edu.wpi.first.wpilibj with parameters of type Relay.Value
`void` | `Relay.set(Relay.Value value)` Set the relay state.
`void` | `Compressor.setRelayValue(Relay.Value relayValue)` Operate the relay for the compressor.

Overview | Package | Class | Use | Tree | Deprecated | Index | Help
| " 2013 FRC Java API "
PREV NEXT | FRAMES NO FRAMES

"
For updated information see the Java FRC site
"