Overview | Package | Class | Use | Tree | Deprecated | Index | Help
| " 2013 FRC Java API "
PREV NEXT | FRAMES NO FRAMES

## Uses of Class
edu.wpi.first.wpilibj.DigitalOutput

Packages that use DigitalOutput
edu.wpi.first.wpilibj | The WPI Robotics library (WPILibJ) is a set of Java classes that interfaces to the hardware in the FRC control system and your robot.

Uses of DigitalOutput in edu.wpi.first.wpilibj

Constructors in edu.wpi.first.wpilibj with parameters of type DigitalOutput
`ADXL345_SPI(DigitalOutput cs, ADXL345_SPI.DataFormat_Range range)` Constructor.
`ADXL345_SPI(DigitalOutput clk, DigitalOutput mosi, DigitalInput miso, DigitalOutput cs, ADXL345_SPI.DataFormat_Range range)` Constructor.
`SPIDevice(DigitalOutput cs)` Create a new device on the SPI bus.
`SPIDevice(DigitalOutput cs, boolean csActiveHigh)` Create a new device on the SPI bus.
`SPIDevice(DigitalOutput clk, DigitalOutput mosi, DigitalInput miso, DigitalOutput cs)` Create a new device on the SPI bus.
`SPIDevice(DigitalOutput clk, DigitalOutput mosi, DigitalInput miso, DigitalOutput cs, boolean csActiveHigh)` Create a new device on the SPI bus.
`Ultrasonic(DigitalOutput pingChannel, DigitalInput echoChannel)` Create an instance of an Ultrasonic Sensor from a DigitalInput for the echo channel and a DigitalOutput for the ping channel.
`Ultrasonic(DigitalOutput pingChannel, DigitalInput echoChannel, Ultrasonic.Unit units)` Create an instance of an Ultrasonic Sensor from a DigitalInput for the echo channel and a DigitalOutput for the ping channel.

Overview | Package | Class | Use | Tree | Deprecated | Index | Help
| " 2013 FRC Java API "
PREV NEXT | FRAMES NO FRAMES

"
For updated information see the Java FRC site
"