Overview | Package | Class | Use | Tree | Deprecated | Index | Help
| " 2013 FRC Java API "
PREV NEXT | FRAMES NO FRAMES

## Uses of Class
edu.wpi.first.wpilibj.GenericHID.Hand

Packages that use GenericHID.Hand
edu.wpi.first.wpilibj | The WPI Robotics library (WPILibJ) is a set of Java classes that interfaces to the hardware in the FRC control system and your robot.

Uses of GenericHID.Hand in edu.wpi.first.wpilibj

Fields in edu.wpi.first.wpilibj declared as GenericHID.Hand
`static GenericHID.Hand` | `GenericHID.Hand.kLeft` hand: left
`static GenericHID.Hand` | `GenericHID.Hand.kRight` hand: right

Methods in edu.wpi.first.wpilibj with parameters of type GenericHID.Hand
`abstract boolean` | `GenericHID.getBumper(GenericHID.Hand hand)` Is the bumper pressed
`boolean` | `Joystick.getBumper(GenericHID.Hand hand)` This is not supported for the Joystick.
`boolean` | `KinectStick.getBumper(GenericHID.Hand hand)` Get the button value for the button set as the default bumper in (@link Joystick)
`abstract boolean` | `GenericHID.getTop(GenericHID.Hand hand)` Is the top button pressed
`boolean` | `Joystick.getTop(GenericHID.Hand hand)` Read the state of the top button on the joystick.
`boolean` | `KinectStick.getTop(GenericHID.Hand hand)` Get the button value for the button set as the default top in (@link Joystick)
`abstract boolean` | `GenericHID.getTrigger(GenericHID.Hand hand)` Is the trigger pressed
`boolean` | `Joystick.getTrigger(GenericHID.Hand hand)` Read the state of the trigger on the joystick.
`boolean` | `KinectStick.getTrigger(GenericHID.Hand hand)` Get the button value for the button set as the default trigger in (@link Joystick)
`abstract double` | `GenericHID.getX(GenericHID.Hand hand)` Get the x position of HID
`double` | `Joystick.getX(GenericHID.Hand hand)` Get the X value of the joystick.
`double` | `KinectStick.getX(GenericHID.Hand hand)` Get the X value of the KinectStick.
`abstract double` | `GenericHID.getY(GenericHID.Hand hand)` Get the y position of the HID
`double` | `Joystick.getY(GenericHID.Hand hand)` Get the Y value of the joystick.
`double` | `KinectStick.getY(GenericHID.Hand hand)` Get the Y value of the KinectStick.
`abstract double` | `GenericHID.getZ(GenericHID.Hand hand)` Get the z position of the HID
`double` | `Joystick.getZ(GenericHID.Hand hand)` Get the Z value of the joystick.
`double` | `KinectStick.getZ(GenericHID.Hand hand)` Get the Z value of the KinectStick.

Overview | Package | Class | Use | Tree | Deprecated | Index | Help
| " 2013 FRC Java API "
PREV NEXT | FRAMES NO FRAMES

"
For updated information see the Java FRC site
"