Overview | Package | Class | Use | Tree | Deprecated | Index | Help
| " 2013 FRC Java API "
PREV NEXT | FRAMES NO FRAMES

## Uses of Class
edu.wpi.first.wpilibj.visa.VisaException

Packages that use VisaException
edu.wpi.first.wpilibj | The WPI Robotics library (WPILibJ) is a set of Java classes that interfaces to the hardware in the FRC control system and your robot.
edu.wpi.first.wpilibj.visa | Provides classes to access I/O functions in visa.h.

Uses of VisaException in edu.wpi.first.wpilibj

Methods in edu.wpi.first.wpilibj that throw VisaException
`void` | `SerialPort.disableTermination()` Disable termination behavior.
`void` | `SerialPort.enableTermination()` Enable termination and specify the termination character.
`void` | `SerialPort.enableTermination(char terminator)` Enable termination and specify the termination character.
`void` | `SerialPort.flush()` Force the output buffer to be written to the port.
`int` | `SerialPort.getBytesReceived()` Get the number of bytes currently available to read from the serial port.
`void` | `SerialPort.print(String write)` Deprecated. use write(string.getBytes()) instead
`byte[]` | `SerialPort.read(int count)` Read raw bytes out of the buffer.
`String` | `SerialPort.readString()` Read a string out of the buffer.
`String` | `SerialPort.readString(int count)` Read a string out of the buffer.
`void` | `SerialPort.reset()` Reset the serial port driver to a known state.
`void` | `SerialPort.setFlowControl(SerialPort.FlowControl flowControl)` Set the type of flow control to enable on this port.
`void` | `SerialPort.setTimeout(double timeout)` Configure the timeout of the serial port.
`void` | `SerialPort.setWriteBufferMode(SerialPort.WriteBufferMode mode)` Specify the flushing behavior of the output buffer.
`int` | `SerialPort.write(byte[] buffer, int count)` Write raw bytes to the buffer.

Constructors in edu.wpi.first.wpilibj that throw VisaException
`SerialPort(int baudRate)` Create an instance of a Serial Port class.
`SerialPort(int baudRate, int dataBits)` Create an instance of a Serial Port class.
`SerialPort(int baudRate, int dataBits, SerialPort.Parity parity)` Create an instance of a Serial Port class.
`SerialPort(int baudRate, int dataBits, SerialPort.Parity parity, SerialPort.StopBits stopBits)` Create an instance of a Serial Port class.

Uses of VisaException in edu.wpi.first.wpilibj.visa

Methods in edu.wpi.first.wpilibj.visa that throw VisaException
`protected static void` | `Visa.assertCleanStatus(String function)`
`static byte[]` | `Visa.viBufRead(int vi, int cnt)`
`static int` | `Visa.viBufWrite(int vi, byte[] buf, int cnt)`
`static void` | `Visa.viClear(int vi)`
`static void` | `Visa.viFlush(int vi, short mask)`
`static int` | `Visa.viGetAttribute(int vi, int attrName)`
`static int` | `Visa.viOpen(int sesn, String name, int mode, int timeout)`
`static int` | `Visa.viOpenDefaultRM()`
`static void` | `Visa.viSetAttribute(int vi, int attrName, boolean attrValue)`
`static void` | `Visa.viSetAttribute(int vi, int attrName, int attrValue)`
`static void` | `Visa.viSetBuf(int vi, short buffer, int size)`
`static void` | `Visa.viVPrintf(int vi, String write)`

Overview | Package | Class | Use | Tree | Deprecated | Index | Help
| " 2013 FRC Java API "
PREV NEXT | FRAMES NO FRAMES

"
For updated information see the Java FRC site
"